FM11 User Manual

**Features：**

* Patented USB rechargeable Multifunctional Flashlight
* Durable stainless steel body
* CREE XP-G2 S4 LED, max output 130 lumens
* Rechargeable 10180 li-ion battery (included)
* Standard Micro USB charging port, chargers in just 1 hour from any USB source
* Charging and fully charged indicator
* 3 mode design, Med/Moonlight/High
* Easy to access to different lighting functions
* Specially designed switch gives easy one-handed operation, and prevents accidental activation
* Magnetic tailcap provides versatile hands free operation
* Headband allows use as headlamp
* Detachable clip
* IPX-8 waterproof

**Specification：**

Emitter: CREE XP-G2

Output & Runtime

|  |  |  |  |
| --- | --- | --- | --- |
| **ANSI/NEMA FL 1** | **High** | **Med** | **Low** |
| Output (lm) | 130 | 14 | 0.2 |
| Runtime | 30mins | 3.4h | 15hours |
| Peak beam intensity(cd) | 431 |
| Max beam distance(m) | 34 |
| Impact resistance(m) | 1.5 |
| Waterproof | IPX8（underwater 2 meters） |

* Length:56.5mm/2.22in

Head diameter: 16.9mm/0.67in

Body diameter：13.2mm/0.52in

* Weight: 32.9g/1.16oz (excluding battery)

Battery:10180 100mAh Li-ion battery

* Working voltage: 3.2V-4.2V
* Accessories: Manual, lanyard, clip, 2\*O-rings and headband

NOTICE: The above-mentioned parameters are approximate and may vary between flashlights, batteries and environments.

**Operation:**

From OFF: 1 click for turn ON

From ON: 1 click for turn OFF

 From ON: Press and hold to cycle through modes (Med/Low/High); release to select brightness level required

**Charging:**

When battery is low, unscrewing the light head and connecting the Micro USB cable to charge as shown in the diagram below

插入充电示意图

**Charging Indicator**

* When charging, the light turns red, when charging is complete, the light turns green. No light indicates that there is no load
* Charging time: 1 hour

**WARNING:**

* Do not point the light at human or animal eyes
* Do not look directly into the light when it is switched on
* Do not permit children to use the flashlight unsupervised

**Warranty Service**

* Guaranteed exchange up to 15 days after purchase: any defective product can be exchanged for a replacement through a local distributor/dealer within 15 days
* After 15 days: all defective products can be repaired free of charge for a period of 2 years from the date of purchase
* Lifetime workmanship guarantee: after the free maintenance period has expired, the maintenance service will charge for material expenses only, free of labor expenses.

**ALTUN LIMITED**

**TEL: +86-755-23764109**

**FAX: +86-755-23760255**

**E-mail:** **info@mecarmy.com**

**Web:** [**www.MecArmy.com**](http://www.mecarmy.com)

**Address:** Yikang Mansion, Huarong Road, Dalang Street, Longhua District, Shenzhen, China